=head1 NAME

App::Netdisco::Manual::Configuration - How to Configure Netdisco

=head1 INTRODUCTION

The configuration files for Netdisco come with all options set to sensible
default values, and just a few that you must initially set yourself.

However as you use the system over time, there are many situations where you
might want to tune the behaviour of Netdisco, and for that we have a lot of
configuration settings available.

=head2 GUIDANCE

There are two configuration files: C<config.yml> (which lives inside Netdisco)
and C<deployment.yml> (which usually lives in C<${HOME}/environments>).

The C<config.yml> file includes defaults for every setting, and should be left
alone.  Any time you want to set an option, use only the C<deployment.yml>
file. The two are merged when Netdisco starts, with your settings in
C<deployment.yml> overriding the defaults from C<config.yml>.

The configuration file format for Netdisco is YAML. This is easy for humans to
edit, but you should take care over whitespace and avoid TAB characters. YAML
supports several data types:

=over 4

=item *

Boolean - True/False value, using C<1> and C<0> or C<true> and C<false>
respectively

=item *

List - Set of things using C<[a, b, c]> on one line or C<-> on separate lines

=item *

Dictionary - Key/Value pairs (like Perl Hash) using C<{key1: val1, key2,
val2}> on one line or C<key: value> on separate lines

=item *

String - Quoted, just like in Perl (and essential if the item contains the
colon character)

=back

=head1 SUPPORTED SETTINGS

=head2 Essential Settings

If you followed the installation instructions, then you should have set the
database connection parameters to match those of your local system. That is,
the database C<name>, C<host>, C<user> and C<pass>.

=head2 General Settings

=head3 C<log>

Value: C<debug|warning|error>. Default: C<warning>.

The log level used by Netdisco. It's useful to see warning messages from the
backend poller, as this can highlight broken topology.

=head3 C<logger_format>

Value: Format String. Default: C<< '[%P] %U %L %m' >>.

Structure of the log messages. See L<Dancer::Logger::Abstract/"logger_format">
for details.

=head3 C<include_paths>

Value: List. Default: Empty List.

Additional library paths for the application (both web frontend and backend
poller daemons). You can also use a colon-separated list in the
"C<NETDISCO_INC>" environment variable.

=head2 Web Frontend

=head3 C<domain_suffix>

Value: String. Default: None.

Set this to your local site's domain name. This is usually removed from node
names in the web interface to make things more readable. Make sure to include
the leading dot character.

=head3 C<no_auth>

Value: Boolean. Default: C<false>.

Enable this to disable login authentication in the web frontend. The username
will be set to C<guest> so if you want to allow extended permissions (C<admin>
or C<port_control>), create a dummy user with the appropriate flag in the
database:

 netdisco=> insert into users (username) values ('guest');
 netdisco=> update users set port_control = true where username = 'guest';
 netdisco=> update users set admin = true where username = 'guest';

=head3 C<navbar_autocomplete>

Value: Boolean. Default: C<true>.

Set this to C<false> to disable the device autocomplete in the main navbar.

=head3 C<suggest_guest>

Value: Boolean. Default: C<false>.

Enable this to display a banner suggesting to log in with a guest account.
The username and password of this account must both be "guest".

=head3 C<trust_remote_user>

Value: Boolean. Default: C<false>.

Enable this if Netdisco is running within another web server such as Apache,
and you want that server to handle user authentication. Normally the
authenticated username will automatically be set in the C<REMOTE_USER>
environment variable. See L<Dancer::Deployment/Running from Apache> for
further details.

=head3 C<trust_x_remote_user>

Value: Boolean. Default: C<false>.

Enable this if you proxy requests to Netdisco via another web server such as
Apache, and you want that server to handle user authentication. You need to
configure the authorized username to be passed from the frontend environment
to Netdisco in the C<X-REMOTE_USER> HTTP Header. For example with Apache:

 RequestHeader unset X-REMOTE_USER
 RequestHeader set X-REMOTE_USER "%{REMOTE_USER}e" env=REMOTE_USER

=head3 C<ldap>

Value: Settings Tree. Default: None.

If set, and a user has the C<ldap> flag also set on their account, then LDAP
authentication will be used for their login.

 ldap:
   servers:
     - 'ad.example.com'
   user_string: 'MYDOMAIN\%USER%'
   opts:
     debug: 3

There are several options within this setting:

=head4 C<servers>

This must be a list of one or more LDAP servers. If using Active Directory
these would be your Domain Controllers.

=head4 C<user_string>

String to construct the user portion of the DN. C<%USER%> is a variable which
will be replaced at runtime with the logon name entered on the logon page of
the application.

Active Directory users may simply use C<MYDOMAIN\%USER%> and skip all other
options except C<servers>, as this notation eliminates the need to construct
the full distinguished name.

Examples: C<cn=%USER%> or C<uid=%USER%>.

=head4 C<base>

Indicates where in the hierarchy to begin searches. If a proxy user is not
defined and anonymous binds are not enabled this value will be appended to the
C<user_string> to construct the distinguished name for authentication.

=head4 C<proxy_user>

User to bind with to perform searches. If defined as C<anonymous>, then
anonymous binds will be performed and C<proxy_pass> will be ignored. For
organizations with users in multiple OUs this option can be used to search for
the user and construct the DN based upon the result.

=head4 C<proxy_pass>

Proxy user password. Ignored if proxy user defined as anonymous.

=head4 C<opts>

Hash of options to add to the connect string. Normally only needed if server
does not support LDAPv3, or to enable debugging as in the example above.

=head4 C<tls_opts>

A hash which, when defined, causes the connection tol use Transport Layer
Security (TLS) which provides an encrypted connection. TLS is the preferred
method of encryption, ldaps (port 636) is not supported.

This is only possible if using LDAPv3 and the server supports it. These are
the options for the TLS connection. See the L<Net::LDAP> documentation under
start_tls for options, but the defaults should work in most cases.

=head3 C<path>

Value: String. Default: None.

Mount point for the Netdisco web frontend. This is usually the root of the web
server. Set this to the path under which all pages live, e.g. C</netdisco2>.
As an alternative you can use the C<--path> option to C<netdisco-web>.

=head3 C<web_plugins>

Value: List of Modules. Default: List of bundled L<App::Netdisco::Web::Plugin> names.

Netdisco's plugin system allows the user more control over the user interface.
Plugins can be distributed independently from Netdisco and are a better
alternative to source code patches. This setting is the list of Plugins which
are used in the default Netdisco distribution.

You can override this to set your own list. If you only want to add to the
default list then use C<extra_web_plugins>, which allows the Netdisco
developers to update default C<web_plugins> in a future release.

Entries in the list will by default omit the leading
C<App::Netdisco::Web::Plugin::> from the name. To override this for one entry,
prefix it with a C<+> sign. You can also prefix with C<X::> to signify the
alternate C<App::NetdiscoX::Web::Plugin::> namepsace.

=head3 C<extra_web_plugins>

Value: List of Modules. Default: Empty List.

List of additional L<App::Netdisco::Web::Plugin> names to load. See also the
C<web_plugins> setting.

=head3 C<reports>

Value: List of Reports Hashes. Default: None.

Use this configuration to add reports to Netdisco without writing any Perl
code or HTML templates. For example:

 reports:
   - tag: power_inventory
     category: Device
     label: 'Power Supply Inventory'
     columns:
       - {name: 'Name'}
       - {ps1_type: 'PS1 Type'}
       - {ps1_status: 'PS1 Status'}
     query: |
       SELECT d.name, d.ps1_type, d.ps1_status
         FROM device d
       ORDER BY name

The C<key> of each item in the C<reports> configuration is an alias for the
report, and becomes part of the web path.

You can munge the data retrieved from the database by placing a Perl script
with the same name as the C<reports> key into the C<site_plugins> directory of
Netdisco's home area. The script can access C<$config> for its configuration
and C<@data> for the retrieved data. It should return a list of munged data.

Within the tree you can provide each of the keys below:

=head4 C<label>

Title for the Report.

=head4 C<columns>

List of single-key Hashes which map database column (field) name to table
heading.

=head4 C<query>

SQL which returns the data. Make sure that the columns are named the same as
the keys of the C<columns> or C<query_columns> configuration. Note the way the
SQL is specified in the example above, using the pipe symbol and then
indenting the query text.

=head4 C<category> (optional)

Section of the Reports menu where this report will appear. See
L<WritingPlugins|App::Netdisco::Manual::WritingPlugins> for the full list.
If not supplied, reports appear in a I<My Reports> category.

=head4 C<query_columns> (optional)

If supplying code to munge the data, the columns returned from your database
C<query> may not be the same as those in the web report. Set this to a list of
the columns in C<query>. The C<columns> setting will then be used for the web
report.

=head3 C<jobqueue_refresh>

Value: Integer Number. Default: 5.

Number of seconds between reloads of the Job Queue panel in the web interface.

=head3 C<safe_password_store>

Value: Boolean. Default: true.

Set to "C<false>" if you MUST maintain backwards compatibility with the Netdisco
1.x web interface. Strongly recommended that you leave this set to "C<true>".

=head3 C<table_pagesize>

Value: Number. Default: 10.

The number of rows in a table page.

=head2 Netdisco Core

=head3 C<mibhome>

Value: Directory. Default: C<${HOME}/netdisco-mibs>.

Base directory in which to find C<mibdirs>. This is where C<netdisco-deploy>
will drop MIB files.

=head3 C<mibdirs>

Value: List of Directories. Default: All subdirectories of C<mibhome>.

A list of subdirectories of C<mibhome> from which to load MIB files. You
should always include C<rfc>. For example:

 mibdirs:
   - rfc
   - cisco
   - foundry

=head3 C<community>

Value: List of Strings. Default: C<public>.

A list of read-only SNMP community strings to try on each device. This is the
simplest way to configure your SNMPv1 or SNMPv2 community strings. For
example:

 community:
   - public
   - anotherstring
   - mycommunity

Each is tried in turn when polling the device, and then the working community
string will be cached in the database.

For fine-grained control over which communities are tried for which devices,
or to set SNMPv3 authentication, see C<snmp_auth>, below.

=head3 C<community_rw>

Value: List of Strings. Default: C<private>.

A list of read-write SNMP community strings to try on each device. The working
community will be cached in the database.

This is the simplest way to configure SNMPv1 or SNMPv2 community strings. Each
is tried in turn when writing to the device, and then the working community
string will be cached in the database.

For fine-grained control over which communities are tried for which devices,
or to set SNMPv3 authentication, see C<snmp_auth>, below.

=head3 C<snmp_auth>

Value: List of Settings Trees. Default: Empty List.

This setting is used for SNMPv3 authentication configuration, and also
provides an alternative fine-grained control for SNMPv1 and SNMPv2 community
strings. You provide a list of authentication stanzas, and Netdisco will try
each in turn, then cache the one which works for a device.

Each stanza can be restricted for use only on specific IP prefixes (subnets),
and also limited to read (get) and/or write (set) operations. By default, a
stanza is enabled for all device IPs, for read access only. The "tag" of a
stanza is simply a friendly name used by Netdisco to refer to the
configuration.

 snmp_auth:
   - community: public
   - communtiy: mycommunity
     write: true
   - community: mycommunity2
     read: false
     write: true
   - tag: v3example
     user: netdisco
     auth:
       pass: netdiscokey
       proto: MD5
     priv:
       pass: netdiscokey2
       proto: DES
   - tag: v3aclexample
     user: netdisco2
     only:
       - 192.0.2.0/30
       - 172.20.10.0/24
   - tag: v2aclexample
     community: s3kr1t
     read: false
     write: true
     only:
       - 2001:db8::/32

For SNMPv1 and SNMPv2, only the C<community> key is required. You can add
C<read> and/or C<write> restrictions, and an IP restriction using C<only>.
Giving the stanza a C<tag> name is optional, but recommended.

For SNMPv3 the C<tag> and C<user> keys are required. You can add C<read>
and/or C<write> restrictions, and an IP restriction using C<only>. Providing
an C<auth> section enables the authentication security level. Providing a
C<priv> section enables the message encryption security level.

As per Net-SNMP, the default SNMPv3 authentication security method is MD5, and
the default encryption protocol is DES, with AES or AES256 being common
alternatives. Note that you cannot have C<priv> without C<auth>.

On some device platforms SNMPv3 contexts are used to macsuck each VLAN. For
this you usually configure a common context prefix, with Netdisco's default
being "C<vlan->" (i.e. C<vlan-1>, C<vlan-2>, etc). Add the C<context_prefix>
key to a stanza to override this.

=head3 C<get_community>

Value: String. Default none.

An external program to run to get the community string for a given device.
This is useful if, for example, you have you devices already configured in
another NMS and you want to use that information instead of configuring
C<snmp_auth>.

The strings "C<%IP%>" and "C<%HOST%>" are replaced by the IP address and the
hostname (or IP address if no hostname is known) of the system being
contacted. For example:

 get_community: '/path/to/my/program %IP%'

The command must return output in the following form:

 community=<comma-separated list of readonly-communities>
 setCommunity=<comma-separated list of write-communities>

If the community string is not known for the given system, the command should
return no output and the community strings configured in C<snmp_auth>,
C<community>, and C<community_rw> will be used instead.

=head3 C<bulkwalk_off>

Value: Boolean. Default C<false>.

Set to C<true> to use C<GETNEXT> instead of the standard C<BULKWALK> for every
device. This will slow things down, but might be necessary for problem
devices. For more fine-grained control see the C<bulkwalk_no> setting.

=head3 C<bulkwalk_no>

Value: List of Network Identifiers or Device Properties. Default: Empty List.

IP addresses in the list will use C<GETNEXT> (and not C<BULKWALK>). You can
include hostnames, IP addresses, subnets (IPv4 or IPv6), YAML Regexp to match
the DNS name, and address ranges (using a hyphen and no whitespace) in the
list.

Alternatively include a "C<property:regex>" entry to match the named property
of the device. The regex must match the complete value.

=head3 C<bulkwalk_repeaters>

Value: Number. Default: 20.

Sets the Net-SNMP C<MaxRepeaters> value, which is used on C<BULKWALK>
operations. See L<SNMP> for more info.

=head3 C<nonincreasing>

Value: Boolean. Default: C<false>.

Setting this to C<true> prevents bulkwalk of device tables with
non-increasing OIDs throwing an error C<OID not increasing> when encountered.
The default is to allow non-increasing OIDs during bulkwalk (which may, in
very badly performing SNMP agents, result in a never-ending loop).  Requires
Net-SNMP 5.3 or higher.

=head3 C<snmpver>

Value: C<1|2|3>. Default: 3.

Highest version of the SNMP protocol used when connecting to devices. Use this
setting to disable SNMP v3 globally. Usually you don't need to configure this.

=head3 C<snmpforce_v1>

Value: List of Network Identifiers or Device Properties. Default: Empty List.

Forces matching devices to use SNMPv1.

=head3 C<snmpforce_v2>

Value: List of Network Identifiers or Device Properties. Default: Empty List.

Forces matching devices to use SNMPv2c.

=head3 C<snmpforce_v3>

Value: List of Network Identifiers or Device Properties. Default: Empty List.

Forces matching devices to use SNMPv3.

=head3 C<snmptimeout>

Value: Number. Default: 1000000.

Micro-seconds before connection retry in L<SNMP::Session>. 1000000
micro-seconds = 1 second.

=head3 C<snmpretries>

Value: Number. Default: 2.

Number of times to retry connecting to a device before giving up.

=head3 C<discover_no>

Value: List of Network Identifiers or Device Properties. Default: Empty List.

IP addresses in the list will not be visited during device discovery. You can
include hostnames, IP addresses, subnets (IPv4 or IPv6), YAML Regexp to match
the DNS name, and address ranges (using a hyphen and no whitespace) in the
list.

Alternatively include a "C<property:regex>" entry to match the named property
of the device. The regex must match the complete value.

=head3 C<discover_only>

Value: List of Network Identifiers or Device Properties. Default: Empty List.

If present, device discovery will be limited to IP addresses matching entries
in this list. You can include hostnames, IP addresses, subnets (IPv4 and
IPv6), YAML Regexp to match the DNS name, and address ranges (using a hyphen
and no whitespace).

Alternatively include a "C<property:regex>" entry to match the named property
of the device. The regex must match the complete value.

=head3 C<discover_no_type>

Value: List of Strings. Default: None.

Place regular expression patterns here to exclude the discovery of certain
devices based on the CDP/LLDP device type information. Good for excluding a
whole device class like lightweight access points or IP phones that have CDP
but don't talk SNMP. For example:

 discover_no_type:
   - 'cisco\s+AIR-LAP'
   - '(?i)Cisco\s+IP\s+Phone'

=head3 C<discover_min_age>

Value: Number. Default: 0.

Sets the minimum amount of time in seconds which must elapse between any two
discover jobs for a device.

=head3 C<macsuck_no>

Value: List of Network Identifiers or Device Properties. Default: Empty List.

IP addresses in the list will not be visited for macsuck. You can include
hostnames, IP addresses, subnets (IPv4 or IPv6), YAML Regexp to match the DNS
name, and address ranges (using a hyphen and no whitespace) in the list.

Alternatively include a "C<property:regex>" entry to match the named property
of the device. The regex must match the complete value.

=head3 C<macsuck_only>

Value: List of Network Identifiers or Device Properties. Default: Empty List.

If present, macsuck will be limited to IP addresses matching entries in this
list. You can include hostnames, IP addresses, subnets (IPv4 and IPv6), YAML
Regexp to match the DNS name, and address ranges (using a hyphen and no
whitespace).

Alternatively include a "C<property:regex>" entry to match the named property
of the device. The regex must match the complete value.

=head3 C<macsuck_all_vlans>

Value: Boolean. Default: C<false>.

Set to macsuck all VLANs, not just the ones that are being used on ports.
This is a debug option. Set this if you think that the option of not
macsucking VLANs that aren't in use on device ports is some how interfering.

=head3 C<macsuck_no_unnamed>

Value: Boolean. Default: C<false>.

Set to true to skip macsuck-ing on VLANs which have no name set. This option
may be useful on Cisco Catalyst family devices where ports are a member of a
VLAN which is not defined in the VLAN database.

=head3 C<macsuck_no_vlan>

Value: List of VLAN names or numbers. Default: fddi-default,
token-ring-default,fddinet-default,trnet-default.

On some devices, per-VLAN macsuck will timeout with specific VLAN numbers. You
can put those numbers (or their names) into this list to have them skipped.

=head3 C<macsuck_no_devicevlan>

Value: List of "IP:vlan-number" or "IP:vlan-name". Default: Empty List.

Similar to C<macsuck_no_vlan>, but allows specifying the device root
(canonical) IP, in order to restrict VLAN skipping only to some devices.

=head3 C<macsuck_bleed>

Value: Boolean. Default: C<false>.

Set to true will let nodes accumulate on uplink ports without topology
information. This is a debug option to help you figure out your topology and
generally should not be set.

=head3 C<macsuck_min_age>

Value: Number. Default: 0.

Sets the minimum amount of time in seconds which must elapse between any two
macsuck jobs for a device.

=head3 C<arpnip_no>

Value: List of Network Identifiers or Device Properties. Default: Empty List.

IP addresses in the list will not be visited for arpnip. You can include
hostnames, IP addresses, subnets (IPv4 or IPv6), YAML Regexp to match the DNS
name, and address ranges (using a hyphen and no whitespace) in the list.

Alternatively include a "C<property:regex>" entry to match the named property
of the device. The regex must match the complete value.

=head3 C<arpnip_only>

Value: List of Network Identifiers or Device Properties. Default: Empty List.

If present, arpnip will be limited to IP addresses matching entries in this
list. You can include hostnames, IP addresses, subnets (IPv4 and IPv6), YAML
Regexp to match the DNS name, and address ranges (using a hyphen and no
whitespace).

Alternatively include a "C<property:regex>" entry to match the named property
of the device. The regex must match the complete value.

=head3 C<arpnip_min_age>

Value: Number. Default: 0.

Sets the minimum amount of time in seconds which must elapse between any two
arpnip jobs for a device.

=head3 C<nbtstat_no>

Value: List of Network Identifiers. Default: Empty List.

IP addresses in the list will not be visited for nbtstat. You can include
hostnames, IP addresses, subnets (nbtstat only supports IPv4), YAML Regexp
to match the DNS name, and address ranges (using a hyphen and no whitespace)
in the list.

=head3 C<nbtstat_only>

Value: List of Network Identifiers. Default: Empty List.

If present, nbtstat will be limited to IP addresses matching entries in this
list. You can include hostnames, IP addresses, subnets
(nbtstat only supports IPv4), YAML Regexp to match the DNS name, and address
ranges (using a hyphen and no whitespace).

=head3 C<nbtstat_max_age>

Value: Number. Default: 7.

The maximum age of a node in days for it to be checked for NetBIOS
information.

=head3 C<nbtstat_interval>

Value: Number. Default: 0.02.

Interval between nbtstat requests in each poller. Defaults to 0.02 seconds,
equating to 50 requests per second per poller.

=head3 C<nbtstat_timeout>

Value: Number. Default: 1.

Seconds nbtstat will wait for a response before time out.  Accepts fractional
seconds as well as integers.

=head3 C<expire_devices>

Value: Number of Days.

Devices that have not been refreshed in this number of days will be removed.
All nodes connected to this device will be removed as well.

=head3 C<expire_nodes>

Value: Number of Days.

Nodes that have not been refreshed in this number of days will be removed from
the database. Archived and non-archived nodes are removed. This includes
SwitchPort/MAC and MAC/IP mappings.

=head3 C<expire_nodes_archive>

Value: Number of Days.

Archived data for switch-port/MAC and MAC/IP mappings older than this number
of days will be removed.

=head3 C<dns>

Value: Settings Tree. Default:

 dns:
   max_outstanding: 50
   hosts_file: '/etc/hosts'
   no: ['fe80::/64','169.254.0.0/16']

After arpnip, each found IP will have its DNS name resolved. Similarly on
device discovery, all interface aliases will have their IPs resolved to names.

This setting controls how many outstanding DNS queries are permitted at any
time. You can also override this setting using the
C<PERL_ANYEVENT_MAX_OUTSTANDING_DNS> environment variable. Similarly, the
location of the Hosts file can be overridden in this config, or using the
C<PERL_ANYEVENT_HOSTS> environment variable.

=head3 C<store_wireless_clients>

Value: Boolean. Default: C<true>.

Set to false to skip the wireless client information gathering. This is
captured at macsuck time, so if you aren't using the information you can skip
it.

=head3 C<store_modules>

Value: Boolean. Default: C<true>.

Set to false to skip the module inventory on device discovery. On some
platforms this can double the discovery time.

=head3 C<ignore_interfaces>

Value: List of Strings. Default:

 ignore_interfaces:
   - 'EOBC'
   - 'unrouted VLAN'
   - 'StackPort'
   - 'Control Plane Interface'
   - 'SPAN (S|R)P Interface'
   - 'StackSub'
   - 'netflow'
   - 'Vlan\d+-mpls layer'
   - 'BRI\S+-Bearer Channel'
   - 'BRI\S+-Physical'
   - 'BRI\S+-Signalling'
   - 'Embedded-Service-Engine\d+\/\d+'
   - 'Virtual-Template\d+'
   - 'Virtual-Access\d+'
   - '(E|T)\d \d\/\d\/\d'

If present, device ports whose names match fully any of the items in this list
will be ignored by the discovery process.

Note this may have side effects - connected devices and nodes on those ports
will in turn also not be discovered.

=head3 C<ignore_private_nets>

Value: Boolean. Default: C<false>.

Set to true to ignore device interfaces that are part of private nets (RFC
1918).

=head3 C<reverse_sysname>

Value: Boolean. Default: C<false>.

Turn this on to have Netdisco do a reverse lookup of the device C<sysName.0>
field to use as the management IP address for a device.

=head3 C<vlanctl>

Value: Boolean. Default: C<true>.

Set to false to prevent users from changing the default VLAN on an interface.
This setting has no effect when C<portctl_nameonly> below is set to true.

=head3 C<portctl_nameonly>

Value: Boolean. Default: C<false>.

Set to true to limit port control action to only changing the interface name
(description).

=head3 C<portctl_nophones>

Value: Boolean. Default: C<false>.

Set to true to make sure an IP Phone port never can be turned off/on.

=head3 C<portctl_vlans>

Value: Boolean. Default: C<false>.

Set to true to allow Netdisco to be able to disable VLAN trunk interfaces.

B<EXTREMELY VERY DANGEROUS>: Turning off a VLAN trunk link could take out most
of your network.

=head3 C<portctl_uplinks>

Value: Boolean. Default: C<false>.

Set to true to allow Netdisco to be able to disable Uplinks. (Router
Interfaces too)

B<EXTREMELY VERY DANGEROUS>: Turning off uplinks will take out chunks of your
network.

=head3 C<check_userlog>

Value: Boolean. Default: C<true>.

Set to false to disable the periodic AJAX check for completed entries in the
job queue for this user. Mainly useful for development to suppress noisy web
frontend activity.

=head3 C<port_control_reasons>

Value: Hash of Strings. Default:

 port_control_reasons:
   address:     'Address Allocation Abuse'
   copyright:   'Copyright Violation'
   dos:         'Denial of Service'
   bandwidth:   'Excessive Bandwidth'
   polling:     'Excessive Polling of DNS/DHCP/SNMP'
   noserv:      'Not In Service'
   exploit:     'Remote Exploit Possible'
   compromised: 'System Compromised'
   other:       'Other'
   resolved:    'Issue Resolved'

When a user has Port Control rights and shuts down a port, they are asked for
a reason. This configuration lists those reasons, and can be overridden to add
or remove any entries.

=head2 Backend Daemon

=head3 C<workers>

Value: Settings Tree. Default:

 workers:
   tasks: 'AUTO * 2'
   sleep_time: 1

Control the activity of the backend daemon with this configuration setting.

C<tasks> sets how many worker processes are started for interactive jobs (port
control) and polling jobs (discover, macsuck, arpnip) on this node. Other
nodes can have different settings.

"C<AUTO>" is the number of CPU cores.  Set C<tasks> to "C<0>" to disable all
workers (which allows you to have a scheduler-only node).

C<sleep_time> is the number of seconds between polling the database to find
new jobs. This is a balance between responsiveness and database load.

=head3 C<dns>

Value: Settings Tree. Default:

 dns:
   max_outstanding: 250
   no: ['fe80::/64','169.254.0.0/16']

Controls the asynchronous DNS resolver used to resolve IP addresses to
names during arpnip and discovery of device aliases.

C<max_outstanding> sets the maximum number of outstanding requests for
asynchronous DNS resolution.  This setting overrides the
C<PERL_ANYEVENT_MAX_OUTSTANDING_DNS> environment value and the C<AnyEvent>
library default of 10.

C<no> is a list of IP addresses or CIDR ranges to excluded from DNS
resolution.  Link local addresses are excluded by default.

=head3 C<schedule>

Value: Settings Tree. Default: None.

If set, then this node's backend daemon will schedule polling jobs (discover,
macsuck, arpnip, etc) in the central database. It's fine to have multiple
nodes scheduling work for redundancy (but make sure they all have good NTP).

Note that this is independent of the Tasks configured in C<workers>. It's
okay to have this node schedule schedule but not do any of the polling
itself (C<tasks: 0>).

Work can be scheduled using C<cron> style notation, or a simple weekday and
hour fields (which accept same types as C<cron> notation). For example:

 schedule:
   discoverall:
     when: '0 9 * * *'
   arpwalk:
     when:
       min: 30
   macwalk:
     when:
       min: 15
       hour: '*/2'
       wday: 'mon-fri'
   nbtwalk:
     when: '0 8,13,21 * * *'
   expire:
     when: '20 23 * * *'

Note that the "C<when>" fields default to "all" (i.e. "C<*>") when not
specified. See L<Algorithm::Cron> for further details.

=head2 Dancer Internal

=head3 C<charset>

Value: String. Default: C<UTF-8>.

See L<Dancer::Config/"charset-string">.

=head3 C<warnings>

Value: Boolean. Default: C<false>.

Should warnings be considered as critical errors?

=head3 C<show_errors>

Value: Boolean. Default: C<false>.

Whether to show a stack trace when an error is caught in the web frontend.

=head3 C<logger>

Value: C<console|file>. Default: C<console>.

Destination for log messages. Should usually be C<console>, which does the
right thing when running foreground apps, and is also captured to
C<${HOME}/logs> when running daemonized. Only change this if you know what
you're doing.

=head3 C<engines>

Value: Settings Tree.

Useful for overriding the Template Toolkit settings, if you want.

=head3 C<layout>

Value: String. Default: C<main>.

Don't touch this.

=head3 C<plugins>

Value: Settings Tree.

Useful for overriding the Database configuration, but only if you know what
you're doing.

=head3 C<session>

Value: String. Default: C<YAML>.

How to handle web sessions. Default is to store on disk so they can be shared
between multiple web server processes (although it's slower).

=head3 C<template>

Value: String. Default: C<template_toolkit>.

Which engine to use for templating in the web frontend. Don't touch this.

=head3 C<route_cache>

Value: Boolean. Default: C<true>.

Whether to build a route cache for web requests, for better performance.

=head3 C<appname>

Value: String. Default: C<Netdisco>.

Don't touch this.

=head3 C<behind_proxy>

Value: Boolean. Default: C<false>.

There's no need to touch this. See deployment documentation for how to proxy.

=head1 UNSUPPORTED (SO FAR)

These settings are from Netdisco 1.x but are yet to be supported in Netdisco
2. If you really need the feature, please let the developers know.

=over 4

=item *

C<col_xxx_show>

=item *

C<macsuck_timeout>

=item *

C<port_info>

=item *

C<portctl_timeout>

=item *

C<timeout>

=back

=cut
